

License # 740020 Since 1997

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Date Rec’d: | | | |  | Scheduled: | |  | | | | | Date completed: | | | |  | | By |  | | |
| Name |  | | | | | | | | | | | Referred By: | | | |  | | By |  | | |
| Product | |  | | | | | | Color | |  | | | | | | Age: |  | Pitch: | | |  |
| Address | | |  | | | | | | | | City | |  | | | | | Zip | |  | |
| Mobile # | |  | | | | Other # | | |  | | | | | E-mail |  | | | | | | |

REV 1/29/15 DOC \_\_\_\_\_\_\_

|  |  |
| --- | --- |
|  | WORK TO BE COMPLETED |
|  | **Leak Repair**: (5-year warranty on area repaired only)   * Pull up \_\_\_ tile over \_\_\_ leaking area(s). Leak location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ * Replace rotten plywood or shiplap, if needed, at no additional cost * Install new synthetic underlayment over leaking area * Reinstall tile and replace any broken tile(s) over the leaking area   **2-year Tune-Up**: (*Umbrella Coverage*: 2-yr leak warranty on the entire roof)   * Replace \_\_\_ broken tile Rake: \_\_\_\_\_\_\_\_ Ridge: \_\_\_\_\_\_\_\_ Type: \_\_\_\_\_\_\_\_\_\_\_\_\_ * Repair \_\_\_ chipped tile * Repair \_\_\_ misplaced tile * Seal \_\_\_ cement crowns with roofing cement and paint to match roof * Seal and paint \_\_\_ vents/pipes * Pull up tile around \_\_\_ chimneys & \_\_\_ skylights, repair tar paper and flashing as needed * Seal and secure exposed nail heads at chimney hood   **5-year Tune-Up**: (*Umbrella Coverage:* 5-yrleak warranty on the entire roof )   * Same as the 2 year tune-up in addition to the following items: * Take out old cement around \_\_\_ vent(s)/pipe(s) * Pull up tile around each vent pipe and repair damaged tar paper as needed * Install new aluminum flashing(s) around each vent/pipe, seal and paint * Re-install existing tile and cut around vent(s)/pipe(s) as needed * Cut 3-in drainage trench in \_\_\_\_ of closed valleys to prevent leaks   **20-year Lift & Re-lay**: (*Umbrella Coverage*: 20-yr leak warranty on the entire roof )   * Pull up \_\_\_ sqrs of tile over the entire roof * Replace rotten plywood or shiplap, if needed, at no additional cost * Install new synthetic underlayment * Install new flashing(s) as needed * Re-install tile and replace any broken tile(s)   7/11/14 |
| **ttl\_amount** | \_\_ Year Transferrable Warranty against leaks on • Entire Roof • Area Repaired |

**TOTAL *3% FEE FOR CREDIT CARD PAYMENTS***

Signature Print Name Date\_\_\_\_\_\_

*By signing here, I authorize The Roof Experts to furnish the services/materials listed here for the above property and agree to pay the cost shown in the “TOTAL” field.*